1. Initializes all variables, left and right whisker=0
2. Left and right motor direction and enable are set for 1
3. If right whisker is hit, set right whisker=1, set left motor direction=0, then reset
4. If left whisker is hit, set left whisker=1, set right motor direction=0, then reset