1. DDRB initial value: 0x00
2. PORTB initial value: 0x00
3. Port B is configured as an output, active high
4. Stack Pointer: 0x10FF
5. Register 0: 0xFF
6. 4 times
7. Register 1: 0xAA
8. Register 2: 0x0F
9. Register 3: 0x0F
10. Stack Pointer in function subroutine: 0x10FD
11. Final results in $0104 and $0105 is 0e and ba

